Intimation no. CTU/N/5/Conn-INT-1A/220000xxx

FORMAT-CONN-INT-1A 
	INTIMATION FOR IN-PRINCIPLE GRANT OF CONNECTIVITY UNDER REGULATIONS 7.1 & 7.2

	A General

	1. 
	Connectivity Intimation No
	:
	

	
	Connectivity Intimation Date 
	:
	

	2. 
	Connectivity Application No.
	:
	

	
	Connectivity Application Date
	:
	

	3. 
	Name of the Applicant
	:
	

	4. 
	Address for Correspondence
	:
	

	5. 
	Location of the Generating Station
Latitude 
Longitude
State
	:
:
:
:
	

	6. 
	Nature of the Applicant
	:
	Generating station(s), including REGS(s), without ESS

	7. 
	Installed Capacity Breakup

	:
	REGS-[Wind  MW ; BESS MW] or
Standalone ESS - MW

[In case of ESS  MWh, No. of cycles] 

	8. 
	SCoD of installed capacity
	
	

	B Connectivity Details

	8.
	ISTS Connectivity details
	:
	

	i. 
	ISTS Connectivity Point
	:
	S/s Name

	ii. 
	Application Type
	
	a) Through separate Bay and DTL
b) Through sharing DTL &Bay of another REGS/RPP with Solar Hour Access

	iii. 
	In case of ii(b), Connectivity Details of entity with Solar Hour Access
	
	· App.  No. 22000xxx
· Connectivity Quantum(MW)
· Injection rights during Solar Hour  MW
· Injection rights during Non Solar Hour MW

	iv. 
	Terminal bay at ISTS end to be constructed under ISTS
	:
	Yes/No

	v. 
	Terminal Bay(s) Voltage level
	:
	220/400/765 kV

	vi. 
	Status of Terminal Bay
	
	Existing/Under Bidding/Under Constr/…etc.

	vii. 
	Bay no. and SLD 
	:
	Bay No xxx

	viii. 
	Non-Solar Hour Access Connectivity Quantum granted (MW) 
	:
	MW

	ix. 
	Injection Rights
	:
	Solar Hour: 0MW
Non-Solar Hour: MW

	x. 
	Maximum Drawl requirement from Grid (In case of REGS with ESS or Standalone ESS)
	
	MW

	xi. 
	Maximum Drawl permitted (In case of REGS with ESS or Standalone ESS)
	
	MW

	xii. 
	Status of ISTS substation 
	:
	Existing/Under Bidding/Under Constr/…etc.

	xiii. 
	Substation Coordinates
	
	Tentative/Final/Not available 

	xiv. 
	Latitude (any point in substation boundary)
	
	

	xv. 
	Longitude (any point in substation boundary)
	
	

	xvi. 
	SCoD of ISTS substation
	
	dd.mm.yyyy(tentative/firm)

	xvii. 
	SCOD of bay at ISTS end, if applicable
	
	dd.mm.yyyy(tentative/firm)

	9.
	Dedicated Transmission Line (DTL)
	:
	

	10.
	ATS/ Augmentation 
	:
	

	10a.
	Associated Transmission System (ATS) Including broad design features
	:
	

	i. 
	Scheme details
	:
	Nil

	ii. 
	Scheduled commissioning date of ATS
	:
	NA

	iii. 
	Estimated Cost of ATS
	:
	NA

	10b.
	Augmentation (Other than ATS)
	:
	

	i. 
	Scheme details
	:
	

	ii. 
	Scheduled commissioning date of Augmentation
	:
	dd.mm.yyyy

	11.
	Start date of Connectivity
	:
	(Tentative: dd.mm.yyyy) 
OR
(Firm : dd.mm.yyyy)

	C Bank Guarantees to be submitted	

	i. 
	Amount of Conn-BG1
	:
	

	ii. 
	Amount of Conn-BG2
	:
	

	iii. 
	Amount of Conn-BG3
	:
	

	D Details of communication system

	i. 
	Details of communication system
	:
	



# Note-1: Regarding S/c line on D/c tower, the applicant shall abide by following terms & conditions: (Applicable in case of S/c on D/c)
1. Implementation of connectivity line on Double Circuit and / or on Multi Circuit towers shall be at own cost & risk of the applicant. 
2. Applicant shall not make any claim for additional bay(s) or additional quantum of injection or overriding priority at ISTS pooling station due to implementation of connectivity line on Double Circuit and / or on Multi Circuit tower. 
3. All issues related to sharing of Double Circuit and / or Multi Circuit towers has to be coordinated among the developers themselves. 
4. Applicant shall not claim any compensation/change in commissioning schedule/Connectivity Start Date/dedicated transmission line completion timeline due to Connectivity line on Double Circuit and /or on Multi Circuit tower. 
Note-2: Connectivity is granted to the ISTS with following terms and conditions:
1. Applicable Conn-BGs shall be furnished within 1 (one) month of this intimation, failing which the application for Connectivity shall be closed, and the application fee shall be forfeited. No extension of time shall be granted to furnish the requisite bank guarantee, and in such case this in-principle grant of Connectivity shall be revoked under intimation to the Connectivity grantee/applicant. In case of applicants under 5.11(a)(ii), upon submission of applicable Conn BGs, the subsisting Conn BGs of original entity (with whom the applicant is sharing DTL & bay) shall be returned on pro-rata basis as per Regulations.
2. During non-solar hours, applicant under 5.11(a) shall be eligible to inject upto the Non-Solar Access Quantum. During the solar hours, the injection rights shall be vested with the entity covered under Regulation 5.11(b) or 5.11(c) as per Regulations.
3. The Grantee shall abide by all provisions and its amendments thereof or re-enactment of:
i) Electricity Act, 2003; 
ii) CERC (Connectivity and General Network Access to the inter-State transmission System) Regulations, 2022 and corresponding Detailed Procedure for Connectivity and GNA; 
iii) CERC (Sharing of Inter-State Transmission Charges and Losses) Regulations, 2020;
iv) CEA (Technical Standards for Connectivity to the Grid) Regulations, 2007 
v) CEA (Technical Standards for construction of Electrical Plants and Electric Lines) Regulations, 2022; 
vi) CEA (Grid Standard) Regulations, 2010; 
vii) CEA (Safety requirements for construction, operation and maintenance of Electrical Plants and Electrical Lines) Regulations, 2011; 
viii) CEA (Measures relating to Safety and Electric Supply) Regulations, 2023;
ix) CEA (Installation and Operation of Meters) Regulations, 2006; 
x) CEA (Technical Standards for Communication System in Power System Operations) Regulations, 2020; 
xi) CERC (Communication System for Inter –State transmission of Electricity) regulations, 2017; 
xii) CERC (Indian Electricity Grid Code) Regulations, 2023.
xiii) CEA (Cyber Security in Power Sector) Guidelines, 2021; 
xiv) CEA (Manual of communication planning in Power System operation), March 2022;
xv) CEA Guidelines for Unified Philosophy for Placement of Phasor Measurement Units (PMUs) in Indian Grid, March 2025;
xvi) Any other applicable Act / Rules / Guidelines / Standards / Regulations / Procedures etc.
4. The applicant shall keep the CTU and RLDC/NLDC indemnified at all times and shall undertake to indemnify, defend and keep the CTU, RLDC/NLDC  harmless from any and all damages, losses, claims and actions including those relating to injury to or death of any person or damage to property, demands, suits, recoveries, costs and expenses, court costs, attorney fees, and; all other obligations by or to third parties, arising out of or resulting from the Connectivity.
5. Towards monitoring of the projects, Connectivity grantee shall comply with Regulations 11 of GNA Regulations 2022, else suitable action shall be taken up as per applicable CERC Regulations. Format for furnishing the progress (through on-line facility) of the project is provided at FORMAT-CONN-STATUS-CG on CTU webportal.
6. (a) For 220kV Lines: Considering Right-of-Way near substation for termination of number of 220kV transmission lines (including Dedicated Transmission Lines), the entities shall coordinate among themselves for implementation of 220kV lines through multi circuit tower near the substation entry for about 2-3 kms stretch. 
Termination of line from multi-circuit tower to substation gantries shall be done using double-circuit dead-end towers, in coordination with the substation developer/developer(s) of other 220kV lines, if required as per site conditions.
(b) For 400kV Lines: Considering Right-of-Way near substation for termination of number of 400kV transmission lines (including Dedicated Transmission Lines), the entities shall coordinate among themselves for implementation of 400kV lines generally through double circuit tower near the substation entry for about 2-3 kms stretch. Further, in case of site constraint with respect to corridor, 400 kV multi circuit may need to be implemented, if required as per inputs of the developer of the ISTS end substation.
(c) As per CEA’s Manual on Transmission Planning Criteria, line approaching substation shall normally be perpendicular to the substation boundary for a stretch of 2-3 kms.
7. Depending on the topology and transmission system requirement, CTU may plan the Connectivity of any generating station(s) at terminal bay of an ISTS substation already allocated to another Connectivity applicant/grantee (such as through Loop-in Loop-out (LILO) of DTL) or at switchyard of a generating station having Connectivity to ISTS for connection and injection of power. In such cases, an agreement (model agreement as per FORMAT-CONN-SHARE) shall be duly signed within one (1) month of the intimation regarding the sharing of DTL and/or terminal bay between the applicants/grantee for sharing the terminal bay / switchyard / dedicated transmission line, failing which the intimations for grant of Connectivity of applicants / grantee shall be liable for revocation.
8. One-time GNA charges shall be applicable as per provisions of Reg 40 & Annexure-IV of GNA Regulations 2022(including amendment)
9. Instruction regarding submission of Technical data for signing of Connectivity Agreement
a) Entity shall comply with CEA (Technical Standards for Connectivity to the Grid) Regulations, 2007 & amendment(s) thereof and shall have to furnish technical data and requisite compliance as per FORMAT-CONN-TD-1 / FORMAT-CONN-TD-2 / FORMAT-CONN-TD-3 (as applicable) of Detailed Procedure to CTU within thirty (30) days from final grant of Connectivity for signing of “Connectivity Agreement viz. FORMAT-CONN-CA-5”.  
b) If the submitted Technical Data is tentative, then the Connectivity Agreement as per FORMAT-CONN-CA-5 shall be signed within thirty (30) days of submission of the tentative Technical Connection Data. In such case, the final technical data shall be provided at least one (1) year prior to physical connection.
c) After receipt of final data, CTU shall scrutinize the submitted data within thirty (30) days and inform regarding discrepancies (if any). Upon rectification of all discrepancies by entity, CTU within thirty (30) days shall intimate the connection details as per FORMAT-CONN-TD-4. Thereafter the Connectivity Agreement as per FORMAT-CONN-CA-5 shall be signed within thirty (30) days. The FORMAT-CONN-TD-4 shall automatically become an integral part of already signed FORMAT-CONN-CA-5. Physical connection to ISTS shall be permitted only after signing of FORMAT-CONN-CA-5.
d) Subsequent to issuance of FORMAT-CONN-TD-4, if there is any change in technical connection data provided by the applicant, it shall submit the revised technical data to CTU with full justification following which CTU shall process the same for revision in FORMAT-CONN-TD-4 within thirty (30) days after receipt of complete data. Such request shall be allowed only once at least three (3) months prior to physical connection to ISTS. However, upon physical interconnection with ISTS, revised technical data, if any, shall be provided to CTU for information and record.


Annexure-I
Transmission system for Connectivity:
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