FORMAT-CONN-INT-2
	INTIMATION FOR ADDITIONAL GENERATION CAPACITY, INCLUDING ESS, WITHIN THE QUANTUM OF CONNECTIVITY GRANTED UNDER REGULATION 5.2

	A General

	1. 
	Intimation No
	:
	

	
	Date
	:
	

	2. 
	Ref. Application No.
	:
	

	
	Date
	:
	

	3. 
	Name of the Applicant
	:
	

	4. 
	Address for Correspondence
	:
	

	5. 
	Location of the Generating Station
Latitude 
Longitude
State
	:
:
:
:
	

	6. 
	Nature of the Applicant
	:
	

	B Connectivity Details

	7. 
	Details for Original Connectivity granted 

	7a 
	Final Intimation No. & date
	:
	

	7b 
	Ref. Application No. & date
	:
	

	7c 
	Installed Capacity(MW) breakup 
	:
	    Solar:  MW
    Wind:  MW
    ESS:   MW

	7d 
	Type of Connectivity:
	
	Solar Hour Access /Non-Solar Hour Access/Full day access

	7e 
	Connectivity Quantum (MW) 
	:
	   MW

	7f 
	Injection Rights
	
	Solar Hour:     MW
Non-Solar Hour:   MW

	7g 
	ISTS sub-station and bay no. of 
	:
	

	7h 
	Firm Start date of Connectivity 
	:
	

	8. 
	Additional Capacity already granted within the Connectivity quantum (MW)
	:
	· App. No. 220000xxx

    Solar:  MW
    Wind:  MW
    ESS:   MW

	9. 
	Additional Capacity granted under present application within the Connectivity quantum (MW)
	
	    Solar:  MW
    Wind:  MW
    ESS:   MW

	10. 
	Total installed capacity [7c+8+9] [MW]
	
	    Solar:  MW
    Wind:  MW
    ESS:   MW

	11. 
	SCoD of additional capacity
	:
	dd.mm.yyyy

	12. 
	Revised Connectivity Quantum (Solar & Non Solar Access) with grant of additional capacity (8 &9)
	
	Solar Hour Access :     MW
Non-Solar Hour Access:   MW

	13. 
	ATS/ Augmentation for drawl
	:
	

	i. 
	Associated Transmission System (ATS) Including broad design features
	:
	

	ii. 
	Scheme details
	:
	

	iii. 
	Scheduled commissioning date of ATS
	:
	

	14. 
	Augmentation (Other than ATS)
	:
	

	i. 
	Scheme details
	:
	

	15. 
	Details of Conn-BGs to be submitted

	(a)
	Conn-BG1
	:
	Rs.  

	(b)
	Conn-BG2
	:
	Rs. (in case of ATS required for drawl)

	(c)
	Conn-BG3
	:
	Rs.  

	12.
	Maximum Drawal from ISTS (MW) (In case of ESS)

	(a)
	Requested by Applicant
	:
	

	(b)
	Granted
	:
	

	C Details of Communication System

	16. 
	Details of Communication System
	:
	



Note: Addition of Generation Capacity is allowed subject to the following terms and conditions:
1. Applicable Conn BGs shall be furnished within 1 (one) month of issuance of this intimation, failing which the application for Connectivity shall be closed, in line with GNA Regulations, 2022. No extension of time shall be granted to furnish the requisite bank guarantee, and in such case the in-principle grant of Connectivity shall be revoked under intimation to the entity.
1. The approval is for addition of generation capacity of (Solar/Wind/ESS____ MW) within the quantum of total Connectivity granted for YYY MW vide intimation referred above. The applicant shall ensure that the net injection at any point of time shall not exceed the quantum of total connectivity granted to M/s XYZ Ltd.  under App. no. 2200000xxx i.e. YY MW. M/s XYZ Ltd (Appl. No. 2200000xxx: YY MW) shall be responsible for compliance with the Grid Code and other regulations of the Central Commission for the above additional generation capacity as ’Lead generator’ in terms of clause (y)(ii) of Regulation 2.1. 
1. The Grantee shall abide by all provisions and its amendments thereof or re-enactment of:
1. Electricity Act, 2003; 
1. CERC (Connectivity and General Network Access to the inter-State transmission System) Regulations, 2022 and corresponding Detailed Procedure for Connectivity and GNA; 
1. CEA (Technical Standards for Connectivity to the Grid) Regulations, 2007 
1. CEA (Technical Standards for construction of Electrical Plants and Electric Lines) Regulations, 2022; 
1. CEA (Grid Standard) Regulations, 2010; 
1. CEA (Safety requirements for construction, operation and maintenance of Electrical Plants and Electrical Lines) Regulations, 2011; 
1. CEA (Measures relating to Safety and Electricity Supply) Regulations, 2023; 
1.  CEA (Installation and Operation of Meters) Regulations, 2006; 
1. CEA (Technical Standards for Communication System in Power System Operations) Regulations, 2020; 
1. CERC (Communication System for Inter –State transmission of Electricity) regulations, 2017; 
1. CERC (Indian Electricity Grid Code) Regulations, 2023;
1. CEA (Cyber Security in Power Sector) Guidelines, 2021; 
1. CEA (Manual of communication planning in Power System operation), March 2022;
1. CERC (Sharing of Inter-State Transmission Charges and Losses) Regulations, 2020
1. CEA Guidelines for Unified Philosophy for Placement of Phasor Measurement Units (PMUs) in Indian Grid, March 2025.
1. Any other applicable Act / Rules / Guidelines / Standards / Regulations / Procedures etc.
1. The entity shall keep the CTU and RLDC/NLDC indemnified at all times and shall undertake to indemnify, defend and keep the CTU, RLDC/NLDC  harmless from any and all damages, losses, claims and actions including those relating to injury to or death of any person or damage to property, demands, suits, recoveries, costs and expenses, court costs, attorney fees, and; all other obligations by or to third parties, arising out of or resulting from the Connectivity.
1. Towards monitoring of the projects, the entity shall comply with Regulations 11 of GNA Regulations 2022, else suitable action shall be taken up as per applicable CERC Regulations. Format for furnishing the progress (through on-line facility) of the project is provided at FORMAT-CONN-STATUS-CG on CTU web portal.
1. Instruction regarding submission of technical data for signing of Connectivity Agreement
1. Entity shall comply with CEA (Technical Standards for Connectivity to the Grid) Regulations, 2007 & amendment(s) thereof and shall have to furnish technical data and requisite compliance as per FORMAT-CONN-TD-1 / FORMAT-CONN-TD-2 / FORMAT-CONN-TD-3 (as applicable) of Detailed Procedure to CTU within thirty (30) days from final grant of Connectivity for signing of “Connectivity Agreement viz. FORMAT-CONN-CA-5”.  
1. If the submitted Technical Data is tentative, then the Connectivity Agreement as per FORMAT-CONN-CA-5 shall be signed within thirty (30) days of submission of the tentative Technical Connection Data. In such case, the final technical data shall be provided at least one (1) year prior to physical connection.
1. After receipt of final data, CTU shall scrutinize the submitted data within thirty (30) days and inform regarding discrepancies (if any). Upon rectification of all discrepancies by entity, CTU within thirty (30) days shall intimate the connection details as per FORMAT-CONN-TD-4. Thereafter the Connectivity Agreement (Cat-2) as per FORMAT-CONN-CA-5-Cat-2 shall be signed within thirty (30) days. The FORMAT-CONN-TD-4 shall automatically become an integral part of already signed FORMAT-CONN-CA-5-Cat-2. Physical connection to ISTS shall be permitted only after signing of FORMAT-CONN-CA-5-Cat-2.
1. Subsequent to issuance of FORMAT-CONN-TD-4, if there is any change in technical connection data provided by the applicant, it shall submit the revised technical data to CTU with full justification following which CTU shall process the same for revision in FORMAT-CONN-TD-4 within thirty (30) days after receipt of complete data. Such request shall be allowed only once at least three (3) months prior to physical connection to ISTS. However, upon physical interconnection with ISTS, revised technical data, if any, shall be provided to CTU for information and record.

Place:									             	ABCD
Date:						                           		CTU Planning
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